Mask aligner



Mask size (diameter):

five inches, four inches

Sample size (diameter):

two inches, four inches, slice (size above 1cm square and below 2 inches in diameter)

We provide S1813 photoresist and standard Micrometer Lithography Process

1,000 NT/Hr